(module easyeda2kicad:HDR-SMD_3P-P2.54-H-F-L11.5 (layer F.Cu) (tedit 5DC5F6A4)
	(attr smd)
	(fp_text reference REF** (at 0 -4.0) (layer F.SilkS)
		(effects (font (size 1 1) (thickness 0.15)))
	)
	(fp_text value HDR-SMD_3P-P2.54-H-F-L11.5 (at 0 4.0) (layer F.Fab)
		(effects (font (size 1 1) (thickness 0.15)))
	)
	(fp_text user %R (at 0 0) (layer F.Fab)
		(effects (font (size 1 1) (thickness 0.15)))
	)
	(fp_line (start 2.54 2.30) (end 2.54 1.27) (layer F.SilkS) (width 0.25))
	(fp_line (start -0.00 2.30) (end -0.00 1.27) (layer F.SilkS) (width 0.25))
	(fp_line (start -2.54 2.30) (end -2.54 1.27) (layer F.SilkS) (width 0.25))
	(fp_line (start 4.01 2.30) (end 4.01 10.86) (layer F.SilkS) (width 0.25))
	(fp_line (start -4.01 10.86) (end 4.01 10.86) (layer F.SilkS) (width 0.25))
	(fp_line (start -4.01 2.30) (end -4.01 10.86) (layer F.SilkS) (width 0.25))
	(fp_line (start -4.01 2.30) (end 4.01 2.30) (layer F.SilkS) (width 0.25))
	(pad 3 smd rect (at 2.54 0.00 0.00) (size 1.00 2.00) (layers F.Cu F.Paste F.Mask))
	(pad 2 smd rect (at 0.00 0.00 0.00) (size 1.00 2.00) (layers F.Cu F.Paste F.Mask))
	(pad 1 smd rect (at -2.54 0.00 0.00) (size 1.00 2.00) (layers F.Cu F.Paste F.Mask))
	(fp_circle (center -4.01 10.80) (end -3.98 10.80) (layer F.Fab) (width 0.06))
	(model "C:/Users/Waldo/Desktop/Blahaj_Pentagramm_Badge/PCB/PCB_Back/easyeda2kicad/easyeda2kicad.3dshapes/HDR-SMD_3P-P2.54-H-F-L11.5.wrl"
		(offset (xyz 0.000 -5.010 -0.000))
		(scale (xyz 1 1 1))
		(rotate (xyz 0 0 0))
	)
)