(module easyeda2kicad:SW-SMD_MK-12C02-G025 (layer F.Cu) (tedit 5DC5F6A4)
	(attr smd)
	(fp_text reference REF** (at 0 -5.58) (layer F.SilkS)
		(effects (font (size 1 1) (thickness 0.15)))
	)
	(fp_text value SW-SMD_MK-12C02-G025 (at 0 5.58) (layer F.Fab)
		(effects (font (size 1 1) (thickness 0.15)))
	)
	(fp_text user %R (at 0 0) (layer F.Fab)
		(effects (font (size 1 1) (thickness 0.15)))
	)
	(fp_line (start 1.30 3.30) (end -0.00 3.30) (layer F.SilkS) (width 0.25))
	(fp_line (start -0.00 3.30) (end -0.00 1.80) (layer F.SilkS) (width 0.25))
	(fp_line (start 1.30 1.80) (end 1.30 3.30) (layer F.SilkS) (width 0.25))
	(fp_line (start 0.09 -0.90) (end -1.59 -0.90) (layer F.SilkS) (width 0.25))
	(fp_line (start 1.59 -0.90) (end 1.41 -0.90) (layer F.SilkS) (width 0.25))
	(fp_line (start 3.20 1.80) (end -3.20 1.80) (layer F.SilkS) (width 0.25))
	(fp_line (start -3.30 0.91) (end -3.30 -0.01) (layer F.SilkS) (width 0.25))
	(fp_line (start 3.30 0.91) (end 3.30 -0.01) (layer F.SilkS) (width 0.25))
	(pad 1 smd rect (at -2.25 -1.58 0.00) (size 0.90 1.80) (layers F.Cu F.Paste F.Mask))
	(pad 2 smd rect (at 0.75 -1.58 0.00) (size 0.90 1.80) (layers F.Cu F.Paste F.Mask))
	(pad 3 smd rect (at 2.25 -1.58 0.00) (size 0.90 1.80) (layers F.Cu F.Paste F.Mask))
	(pad 4 smd rect (at 3.80 -0.69 0.00) (size 1.10 0.93) (layers F.Cu F.Paste F.Mask))
	(pad 5 smd rect (at 3.80 1.58 0.00) (size 1.10 0.93) (layers F.Cu F.Paste F.Mask))
	(pad 6 smd rect (at -3.80 1.58 0.00) (size 1.10 0.93) (layers F.Cu F.Paste F.Mask))
	(pad 7 smd rect (at -3.80 -0.69 0.00) (size 1.10 0.93) (layers F.Cu F.Paste F.Mask))
	(pad "" thru_hole circle (at 1.50 0.45) (size 0.85 0.85) (drill 0.85) (layers *.Cu *.Mask))
	(pad "" thru_hole circle (at -1.50 0.45) (size 0.85 0.85) (drill 0.85) (layers *.Cu *.Mask))
	(fp_circle (center -3.85 -1.91) (end -3.82 -1.91) (layer F.Fab) (width 0.06))
	(fp_circle (center -1.50 0.45) (end -1.30 0.45) (layer Cmts.User) (width 0.40))
	(fp_circle (center 1.50 0.45) (end 1.70 0.45) (layer Cmts.User) (width 0.40))
	(model "${EASYEDA2KICAD}/easyeda2kicad.3dshapes/SW-SMD_MK-12C02-G025.wrl"
		(offset (xyz -0.000 -0.690 -0.000))
		(scale (xyz 1 1 1))
		(rotate (xyz 0 0 0))
	)
)