(footprint "KH-6X6X6H-STM"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 4.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "4fc5d222-e60e-4834-8130-25692e817f4f")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "KH-6X6X6H-STM"
		(at 0 6 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "2eea9311-7b93-45da-82a9-9bb11c277846")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4f66d8ee-772f-46e8-a8b7-5076733c997d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2c6032a4-5423-4979-b580-4bc9c86302ab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3001b86a-b5d3-44b3-ae92-3b207376b203")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -3 -3)
		(end 3 -3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ce9de524-10c7-4108-9cee-cd9e94fa9fdc")
	)
	(fp_line
		(start -3 3)
		(end -3 -3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "1adfd3ac-e8ea-4743-a5e0-828794876ae0")
	)
	(fp_line
		(start -2.5 3)
		(end -3 3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f3e28d67-298f-453c-b7f7-94b0a2a9ab3f")
	)
	(fp_line
		(start 3 -3)
		(end 3 3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "189f4086-a0a2-4c3f-bb49-9c7b168af4be")
	)
	(fp_line
		(start 3 3)
		(end -2.5 3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "263082dc-5f2c-411c-b52b-4a983712c691")
	)
	(fp_text user "${REFERENCE}"
		(at 0 7.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c4182631-cfe2-450c-a401-004644e3f73b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -5 -2.25)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "9e8e4fdd-861c-4d85-85d3-0f16d7bb8933")
	)
	(pad "2" smd rect
		(at 5 -2.25)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "178c5cdc-8d4a-43e6-9274-3bdabdc530d4")
	)
	(pad "3" smd rect
		(at -5 2.25)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "b0a34bf8-7ce6-4e1a-8d8b-5c9e4482fd59")
	)
	(pad "4" smd rect
		(at 5 2.25)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "0813121a-7ef2-4f41-ae8a-1906ed0a30d1")
	)
)